FOX MONITOR 2
By ORION
Instruction:
To install it, load up the code you want to investigate, then load the 'FOX MON'. It lives in screen memory, so as not to clash with the code you're examining.
Controls:
‘Q’	- return to Basic
‘W’	- set a trap
‘R’	- start running the code
‘T’	- insert text
‘I’	- memory block operations
‘O’	- insert Poke (SPACE to exit)
‘P’	- printer (destroys the printer buffer)
‘A’	- change mode (text/assembler)
‘S’	- save
‘D’	- math operations (+/-)
‘F’	- text searching
‘G’	- bytes searching (press ENTER twice to start)
‘H’	- change mode (hex/dec)
‘J’	- load
‘L’	- move memory block
‘B’	- binary conversion
‘N’	- next address (when using ‘F’ or ‘G’)
‘M’	- set address
‘5’, ‘6’, ‘7’, ‘8’ - moving through the memory
Additional information:
When entering data by INPUT, use ‘#’ before a hex number.  If you press ENTER the value will be 0.  If you have a TIMEX FLOPPY DISK use ‘CAPS SHIFT’+ ‘J’ for load and ‘CAPS SHIFT’+ ‘S’ for save.