FILE COMPRESSOR V1.9
After loading the keys letters are highlighted: L, C, N, T, H, D -> only for tape/Timex TOS FDD.  Lets say the main code of the game is at 24576, length 35000.  Load it by L option.  After loading press C to compress; the address must be lower than main code address (e.g. 24500) then the program after having compressed the code asks whether you want to save the compressed file or not and then asks for the new name.  After saving you have to add into the BASIC loader: CLEAR address of compression-1, (in our example 24499), and then before last USR command insert RANDOMIZE USR address of compression (in ours e.g. 24500).
The old loader (example):
CLEAR 24575
LOAD “” SCREEN$
LOAD “” CODE
RANDOMIZE USR 35000
The new loader (our example):
CLEAR 24499
LOAD “” SCREEN$
LOAD “” CODE
RANDOMIZE USR 24500 – decompress
RANDOMIZE USR 35000