MAD MONITOR 2
Instruction:
To install it, load up the code you want to investigate, then load the 'FOX MON'. It lives in screen memory, so as not to clash with the code you're examining.
Controls:
‘Q’	- return to Basic
‘W’	- set a trap
‘R’	- start running the code
‘P’	- insert Poke (address, value)
‘S’	- save
‘D’	- conversion dec->hex
‘G’	- bytes searching (press ENTER twice to start)
‘H’	- conversion hex->dec
‘J’	- load
‘L’	- ASCII display (X – exit)
‘N’	- next address (when using ‘G’)
‘M’	- set address
‘5’, ‘6’, ‘7’, ‘8’ - moving through the memory
‘1’	- registers, I change value, X exit